Method: Tftp tool
Please download tftpd on you pc or laptop which have an Ethernet port and which will be used to restore the router
1. Power the node off first
2. press the reset button while power on the node for 20-25 seconds. (hold on for 20-25 seconds)
[bookmark: OLE_LINK1]2. connect 5G01 lan port with PC, configure IP address of PC to 192.168.1.10
3. open tftp on PC (Please make sure turn off the firewall)
[image: ]
[image: getComposeData&sid=BAQKRNVVemnjqhjNbaVVcLRsxREQbUxn&composeId=1494829366914&attachId=2]
Attention
· Current Directory: please keep default.
· Server interfaces: please select network card with 192.168.1.10
· Click DHCP server without configuration, click Tftp Client, enter 192.168.1.6 in Host
· Local File means the firmware you are going to upgrade, click “…”to select the firmware in tftp file.
Click “PUT” button,the page will be showed as below, click ok.
[bookmark: _GoBack][image: getComposeData&sid=BAQKRNVVemnjqhjNbaVVcLRsxREQbUxn&composeId=1494829366914&attachId=3]
4. If the process was successful and there were no errors, wait up to 2 minutes and disconnect your router from the computer and try to reboot it. Next, check if it is working properly.


image1.png
R 2013/11/2..  thpd32 RIFEERF 211KB




image2.png
Tftpd32 by Ph. Jounin

et Diretory <l Bowse
Serverinteaces (152 168 1841 VMware Vi v| _ ShowDit
Tt Clent | GHCP corver-Log yiwer |

Host [19276616 Pat
LocalFile  |hHEU t_BAD_M.bin

Remate File
Block [Default_v.
Size
Get | | Put
About Setlings

Help





image3.png
1£tpd32

0 block retransnitted
WIS 23c0e abb 32865 4788 «34:31 82436848

5V)

.





